**TVR alarm 3 button remote instructions.**

**To lock vehicle & arm alarm** press the right button once, indicators will flash twice & alarm status LED will flash for 30 seconds, pause then flash at a slower rate. Alarm is now fully armed and vehicle is locked.

*Within this 30 second think time the alarm is not fully armed its just checking the doors & internal sensors. If any of these are triggered during this time it will trigger the indicators & flash once with single beep from the siren each time it sees a trigger.*

**If you hear 4 low tones from the siren when locking the vehicle this is a warning & means that the alarm is seeing a door, boot or bonnet open.**

***N.B. Tuscan, Tamora, T350 & Sagaris.***

*If you hear this its often the alarm picking up a signal from the door locking control ecu’s, to avoid this you can wait for 30 seconds after closing the doors before pressing the button. This allows the ecu’s to finish their locking/ window closing cycle.*

**To lock the vehicle & disable the internal sensor & tilt sensor,** press the right button once wait for the indicator flashing cycle to finish then press the same button 3 times the indicators will flash 5 times with 5 beeps. Please note that the alarm status LED will flash rapidly for the remaining think time to indicate that the system has been armed with the sensors disabled. **N.B. this is not available for Cerbera**

**To unlock and disarm alarm press left hand button once,** this will disarm the alarm & unlock the doors.

**If you hear a low tone when you disarm the vehicle this means that the alarm has been triggered in your absence. The alarm via the alarm status LED will indicate to you what sensor was triggered. It does this by flashing the LED in a sequence then waits for around 10 seconds, then repeats the same sequence. It will continue to do this until either the ignition has been turned on or the alarm is armed again.**

**1: Flash = Ultrasonics**

**2: Flashes = Doors**

**3: Flashes = Boot or Bonnet**

**4: Flashes = Boot or Bonet**

**5: Flashes = Microwave (internal sensor)**

**6: Flashes = Ignition (turned on)**

**7: Flashes = Tilt sensor**

**When pressing the boot function it is recommended that is always done when the alarm is in its disarmed state & vehicle is unlocked.**