**How to Program QYT KT-8900**

**Basic Instructions using Speaker Microphone:**

Press [F Key] + [# Key] + [# Key]

***Select value***

Press [F Key] to save it

Press [Exit/AB]

A screenshot of a computer

AI-generated content may be incorrect.

A screenshot of a computer

AI-generated content may be incorrect.

A screenshot of a computer

AI-generated content may be incorrect.

A screenshot of a computer

AI-generated content may be incorrect.

**1. Start in VFO mode.**

**2. Punch in Transmit frequency**

**3. CTCSS Tone on Transmit side – 13 (**TX CTCSS)

**4. Shift Direction - 38**

**5. Shift Value – 39**

**How to Program QYT KT-8900**

**Basic Instructions using Speaker Microphone:**

Press [F Key] + [# Key] + [# Key]

***Select value***

Press [F Key] to save it

Press [Exit/AB]

A screenshot of a computer

AI-generated content may be incorrect.

A screenshot of a computer

AI-generated content may be incorrect.

A screenshot of a computer

AI-generated content may be incorrect.

A screenshot of a computer

AI-generated content may be incorrect.

**Programming a Repeater**

1. Start in VFO mode.

2. Punch in Transmit frequency

3. CTCSS Tone on Transmit side – 13 (TX CTCSS)

4. Shift Direction - 38

5. Shift Value – 39