**How to Program the TYT-9800**

**Basic Instructions:**

Short press the [SET] key to enter Menu Mode

Rotate the Main band **DIAL** to select Menu #

Short press the Main band **DIAL**

Rotate Main band DIAL for selection

Short press [SET] to save setting

**1. Start in VFO mode.**

**2. Punch in Transmit frequency**

**3. CTCSS Tone on Transmit side - 30**

TX CTCSS

Function

Type in tone

**4. Shift Direction - 38**

Use knob or up and down buttons

Function

Type in tone

**5. Shift Value - 27**

Type value

Function

Type in tone

**6. Channel # - 36**

Enter with knob

**7. Saving the Channel**

In VFO mode, enter receive frequency (Transmit frequency + shift)

Function

Channel #

Function

**8. Channel Name - 18**

In Channel mode, select channel

Turn dial for letter - #/Lock button - Repeat for following letters