**Maxess FlexFit**

Non-rated Plastic Access Panel

For installations in walls and ceilings



|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **CODE** | **SIZE** | **WEIGHT** | **A** | **B** | **C** | **D** | **E****MAX OPENING****SIZE (H-H)** | **F** | **G****MIN.****OPENING****SIZE (J-J)** | **MIN.****SPRING** **TENSION** | **MAX****SPRING****TENSION** |
| **APF 8** | **8”** | ½ LB230 G | 10”x10”254x254MM | 6”x6”150x150MM | 1”25.4MM | 9 ½”240MM | 8¾“x8¾“220x220MM | 6”150MM | 6” x 6”150x150MM | 2 LB1000 GAT MAXOPENING | 5 LB2500 GAT MINOPENING |
| **APF12** | **12”** | 1 LB450 G | 14”x14”355x355MM | 10”x10”254x254MM | 1”25.4MM | 13.5”343MM  | 12¾“x12¾“324x324MM | 10”254MM | 10”x10”254x254MM | 2 LB1000 GAT MAXOPENING | 5 LB2500 GAT MINOPENING |

**MATERIAL:** HIGH IMPACT STYRENE

**FINISH:** TEXTURED OUTER SURFACE

**COLOR:** WHITE

**PROPERTY OF:** NOVERA PRODUCTS INC. [www.noveraproducts.ca](http://www.noveraproducts.ca)