|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Address: | Room: | Name of surveyor: | Signature: | Sheet no.: |
| RF Meter Make: | ELF Meter Make: | Appliances with RFR / EMF: |
| ***ZERO IGNIR COMPLIANCE: above Day Max*** | ***DAY*** | ***NIGHT*** | ***SENSITIVE*** | *Circle appropriate level:****IGNIR COMPLIANCE******Zero****/* ***Day****/* ***Night****/* ***Sensitive*** |
| **IGNIR** | **Reading** | **Date** | **Time** | **IGNIR** | **Reading** | **Date** | **Time** | **IGNIR** | **Reading** | **Date** | **Time** |
| **RF** | *V/m* | Av. |  0.06 |  |  |  |  0.02 |  |  |  | ≤0.006 |  |  |  | **Z/D/N/S** | Av. | *V/m* | **RF** |
| **Max** |  **0.2**  |  |  |  |  **0.06** |  |  |  |  **≤ 0.02** |  |  |  | **Z/D/N/S** | **Max** |
| *µW/m2* | Av. | 10 |  |  |  | 1 |  |  |  | 0.1 |  |  |  | **Z/D/N/S** | Av. | *µW/m2* |
| **Max** | **100** |  |  |  | **10** |  |  |  | **1** |  |  |  | **Z/D/N/S** | **Max** |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **VLF** | *G-S Units* | **Max** | **120** |  |  |  | **70** |  |  |  | **30** |  |  |  | **Z/D/N/S** | **Max** | *G-S Units* | **VLF** |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **ELF** | *V/m* | Av. | 10 |  |  |  | 3 |  |  |  | 1 |  |  |  | **Z/D/N/S** | Av. | *V/m* | **ELF** |
| *nT* | Av. | 300 |  |  |  | 100 |  |  |  | 30 |  |  |  | **Z/D/N/S** | Av. | *nT*  |
| **Max** | **1000** |  |  |  | **300** |  |  |  | **100** |  |  |  | **Z/D/N/S** | **Max** |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | **©** *IGNIR* |

 **IGNIR COMPLIANCE FORM** *Supplement 3*

*Sketch the room overleaf or on a separate sheet of paper. Mark areas in appropriate colour****RED – Zero IGNIR compliance****,* ***BROWN – Day compliance,*** *GREEN – Night compliance, or BLUE – Sensitive compliance.*

*Sketch of the room, Mark areas in appropriate colours for IGNIR compliance:*

***RED – Zero IGNIR compliance****,* ***BROWN – Day compliance,*** *GREEN – Night compliance, or BLUE – Sensitive compliance.*