**How to Program Baofeng HTs**

**Basic Instructions:**

Press Menu

Use the Up and Down keys to navigate

Press Menu

Set the parameter

Press Menu to save & return to main Menu

Press Exit

**1. Start in VFO mode.**

**2. Punch in Transmit frequency**

**3. CTCSS Tone on Transmit side - 13**

TX CTCSS

Press Menu

Type in tone

**4. Shift Direction - 25**

Use knob or up and down buttons

Press Menu

Type in tone

**5. Shift Value - 26**

Type value

Press menu

Type in tone

**6. Channel # - 27**

Enter with knob

**7. Saving the Channel**

In VFO mode, enter receive frequency (Transmit frequency + shift)

Press Menu

Channel #

Press Menu